**Section 860.280 Lighting**

Communities constructed after July 1, 1998 shall have an average illumination level of at least 0.6 foot candles and a minimum illumination level of 0.3 foot candles maintained for all streets in the manufactured home community. (Type A Violation)

(Source: Amended at 43 Ill. Reg. 2558, effective February 6, 2019)