**Section 890.310 Tightness**

Joints and Connections. Joints and connections shall be gas-tight and water-tight.