**Section 890.1020 Material and Size**

Indirect waste pipe sizes shall be the same as the fixture outlets, but at least three-fourths (3/4) inch.