**Section 890.1060 Special Wastes and Chemical Wastes**

a) Acid Wastes. Acid and chemical waste piping and fittings, including the trap, shall be of material that will not be damaged by the waste being discharged.

b) Neutralizing Device. Corrosive liquids, spent acids, or other harmful chemicals shall not be discharged into the building sewer without first being properly diluted or neutralized.