**Section 905.APPENDIX A Illustrations and Exhibits**

**Section 905.ILLUSTRATION S Chlorine Contact Tank**

**Section 905.EXHIBIT A Minimum Required Chlorine Contact Tank Volume**

|  |  |
| --- | --- |
| AVERAGE FLOW RATEGPD | MINIMUM REQUIRED VOLUMEGALLONS |
| 100 | 30 |
| 200 | 30 |
| 300 | 30 |
| 400 | 30 |
| 500 | 30 |
| 600 | 30 |
| 700 | 36 |
| 800 | 42 |
| 900 | 47 |
| 1000 | 52 |
| 1100 | 57 |
| 1200 | 63 |
| 1300 | 68 |
| 1400 | 73 |
| 1500 | 78 |

**Section 905.APPENDIX A Illustrations and Exhibits**

**Section 905.ILLUSTRATION S Chlorine Contact Tank**

**Section 905.EXHIBIT B Chlorine Feeder, Contact Tank, and Sampling Port**



(Source: Amended at 20 Ill. Reg. 2431, effective March 15, 1996)