**Section 737.600 Construction and Maintenance**

a) Each Local Provider shall place a minimum of 80% of all newly constructed outside cable plant facilities (measured in sheath miles) underground.

b) The telecommunications outside plant shall be designed, constructed, maintained and operated in accordance with the provisions of 83 Ill. Adm. Code 305 and 83 Ill. Adm. Code 265.

(Source: Amended at 39 Ill. Reg. 364, effective December 22, 2014)