**Section 1328.310 Authorized Wireless 9-1-1 Answering Point Testing**

Ongoing testing after the authorized wireless 9-1-1 answering point is on-line shall include the following:

a) Testing with all wireless carriers, including, but not limited to, the 9-1-1 database, network trunking, system overflow, system backup, default routing, and call transfers, on an annual basis. The mutually agreed upon testing shall be coordinated in advance by the 9-1-1 authority and the participating wireless carriers.

b) Coordinated testing with the participating wireless carriers when any of the following occurs:

1) New mobile switching office installations;

2) NPA and NXX pANI additions;

3) Local number portability implementations;

4) Number pooling implementations; and

5) Any other event that affects 9-1-1.