**Section 14.740 Facilities**

Every RLA shall provide:

a) Wind direction/velocity indicator (must be lighted for night use); and

b) Clearly marked thresholds and/or displaced thresholds visible from 1500' above ground level (AGL) as shown in Appendix E, Illustration E.

(Source: Amended at 38 Ill. Reg. 20064, effective October 2, 2014)