**Section 442.455 Horn**

The bus shall be equipped with at least one horn *capable of emitting sound audible under normal conditions from a distance of not less than 200 feet.* (Section 12-601 of the Code) The horn shall be conveniently controlled from the operator’s position and tested in accordance with SAE Standard J377.

(Source: Amended at 31 Ill. Reg. 8238, effective May 25, 2007)