**Section 550.ILLUSTRATION B Table of Entrance Layout Requirements**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | NONCOMMERCIAL RURAL | NONCOMMERCIAL URBAN | COMMERCIAL RURAL | | COMMERCIAL URBAN | INDUSTRIAL-COMMERCIAL-RECREATIONAL HGH-VOLUME TRAFFIC GENERATORS |
| WIDTH OF DRIVE | 12' Min.  24' Max. | | 35' Max.  (60' Max. 6' from Edge of Pavement) | | 35' Max.  (85' Max. at Curb) | 2@24'  or 35' Max. |
| RADII OF FLARE | 10' Min.  30' Max. | 5' Min.  15' Max. | 10' Min.  40' Max. | | 10' Min.  25' Max. | 30 – 50'  or 3 C.C. |
| ANGLE OF DRIVE | 60º - 90º | \*45º - 90º | | | | |
| ISLAND AREA | ---- | | 10' Min. at ROW  5' Min. Radius  10' Min 6' from Pavement | | 6' Min. at Edge of Pavement and at ROW  5' Min. Radius | 4' – 18" Wide Median |
| DISTANCE FROM PROPERTY LINE (To any part of driveway or flare) | 0' Min. | | 5' Min.  (6' from Edge of Pavement) | | 3' Min. | 10' Min. |
| DISTANCE FROM INTERSECTING STREET | \*\*50' Min. | \*\*\*5' Min. | \*\*50' Min. | | ---- | \*\*100' Min. |
| 5' Min. from beginning of flare to extension of intersecting road ROW | | | | |
| DISTANCE BETWEEN DRIVES | ---- | | | 10' Min.  (6' from Edge of Pavement and at ROW) | 6' Min.  (at Edge of Pavement and at ROW) | 440' Min.  660' Desirable |

\* 45º permitted only for one-way drives; 60º minimum for two-way drives.

\*\* From edge of intersecting road to beginning of driveway flare.

\*\*\* Undisturbed length of curb between driveway flare and intersecting street flare.