**Section 550.ILLUSTRATION H Typical Left-Turn Lane on Two-Lane Highway**



Note 1 – Distances shown are based on 50 mph design speed.

Note 2 – Double yellow thermoplastic or painted median diagonals.

12-inch lines with spacing as indicated in Section 3-3.8 of MUTCD.

Note 3 – Increased if necessary for storage requirements.

Note 4 – In rural areas, 500-foot minimum no-passing zone should be marked on approaches.