**Section 557.130 Walking On or Along a Roadway (Type I Hazard)**

In determining whether a pupil walking on or along a roadway is endangered by a serious safety hazard, the location of a pupil in relation to the roadway, speed and volume of traffic, and length of hazardous section will be considered. To determine whether a serious safety hazard exists in a particular situation, appropriate points from subsections (a) and (b) will be added together.

a) Type and Length of Hazardous Section

|  |  |  |
| --- | --- | --- |
| LOCATION OF PUPIL | LENGTH | POINTS |
| On roadway for a minimum of 50' because of narrow bridge or overpass | 50' - 100'  100' - 200'  More than 200' | 7 points  9 points  10 points |
| On roadway for a minimum of 300' because of no shoulder or sidewalk | 300' - 1000'  1000' - 2000'  More than 2000' | 7 points  9 points  10 points |
| On narrow shoulder within 5' of roadway for a minimum of 0.2 mile | 0.2 - 0.5 mile'  0.5 - 1 mile  More than 1 mile | 6 points  8 points  10 points |

b) Speed and Volume of Traffic

|  |  |  |
| --- | --- | --- |
| SPEED | VOLUME | POINTS |
| 50 - 55 mph | Heavy  Moderate  Light | 8  6  4 |
| 40 - 45 mph | Heavy  Moderate  Light | 6  4  2 |
| 30 - 35 mph | Heavy  Moderate  Light | 5  3  1 |