**Section 557.130 Walking On or Along a Roadway (Type I Hazard)**

In determining whether a pupil walking on or along a roadway is endangered by a serious safety hazard, the location of a pupil in relation to the roadway, speed and volume of traffic, and length of hazardous section will be considered. To determine whether a serious safety hazard exists in a particular situation, appropriate points from subsections (a) and (b) will be added together.

a) Type and Length of Hazardous Section

|  |  |  |
| --- | --- | --- |
| LOCATION OF PUPIL | LENGTH | POINTS |
| On roadway for a minimum of 50' because of narrow bridge or overpass | 50' - 100'100' - 200'More than 200' | 7 points9 points10 points |
| On roadway for a minimum of 300' because of no shoulder or sidewalk | 300' - 1000'1000' - 2000'More than 2000' | 7 points9 points10 points |
| On narrow shoulder within 5' of roadway for a minimum of 0.2 mile | 0.2 - 0.5 mile'0.5 - 1 mileMore than 1 mile | 6 points8 points10 points |

b) Speed and Volume of Traffic

|  |  |  |
| --- | --- | --- |
| SPEED | VOLUME | POINTS |
| 50 - 55 mph | HeavyModerateLight | 864 |
| 40 - 45 mph | HeavyModerateLight | 642 |
| 30 - 35 mph | HeavyModerateLight | 531 |