**Section 351.APPENDIX B Example of Plaque for Identifying Wells Containing Sealed Sources Containing Radioactive Material Abandoned Downhole**

[COMPANY NAME]

[WELL IDENTIFICATION]

 **CAUTION** 

ONE 74 GIGABECQUEREL (2 CURIE)

CS-137 RADIOACTIVE SOURCE

ABANDONED 3-3-92 AT 2560

METERS (8400 FEET) PLUG BACK

DEPTH 2500 METERS (8200 FEET)

DO NOT RE-ENTER THIS WELL

BEFORE CONTACTING THE

 ILLINOIS EMERGENCY

MANAGEMENT AGENCY

The size of the plaque should be convenient for use on active or inactive wells, e.g., a 17-centimeter (7-inch) square and 3 mm (⅛ inch) thick. Letter size of the word "CAUTION" should be approximately twice the letter size of the rest of the information, e.g., 12-millimeter (½-inch) and 6-millimeter (¼-inch) letter size, respectively. Quantities and distances may be expressed either in SI units or in special and English units or in dual units.