**Section 211.890 Capture**

"Capture" means the containment or recovery of emissions from an emission unit for direction into a duct which may be exhausted through a stack or vent to a control device. The overall abatement of emissions from an emission unit with an add-on control device is a function both of the capture efficiency and of the control device efficiency.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)