**Section 211.995 Circulating Fluidized Bed Combustor**

"Circulating fluidized bed combustor" means, for purposes of Part 217, a fluidized bed combustor in which the majority of the fluidized bed material is carried out of the primary combustion zone and is transported back to the primary zone through a recirculation loop.

(Source: Added at 33 Ill. Reg. 13326, effective August 31, 2009)