**Section 211.1150 Closed Vent System**

"Closed vent system" means a system that is not open to the atmosphere and is composed of piping, connections, and, if necessary, flow inducing devices that transport gas or vapor from a piece or pieces of equipment to a control device.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)