**Section 211.2960 High-Performance Architectural** **Coating**

"High-performance architectural coating" means, for purposes of 35 Ill. Adm. Code 218 and 219, a coating used to protect architectural subsections and that meets the requirements of the Architectural Aluminum Manufacturer Association's publication number AAMA 2604-05 (Voluntary Specification, Performance Requirements and Test Procedures for High Performance Organic Coatings on Aluminum Extrusions and Panels), incorporated by reference in Section 211.101 of this Part, or 2605-05 (Voluntary Specification, Performance Requirements and Test Procedures for Superior Performing Organic Coatings on Aluminum Extrusions and Panels), incorporated by reference in Section 211.101 of this Part.

(Source: Added at 34 Ill. Reg. 14119, effective September 14, 2010)