**Section 211.2990 High Volume Low Pressure (HVLP) Spray**

"High volume low pressure (HVLP) spray" means equipment used to apply coatings by means of a spray gun which operates between 0.1 and 10 psig air pressure.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)