**Section 211.4830 Polyester Resin Material(s)**

"Polyester resin material(s)" means gel coat and unsaturated polyester resin, such as isophthalic, orthophthalic, halogenated, bisphenol A, vinyl ester, or furan resins; cross-linking agents; catalysts; inhibitors; accelerators; promoters; and any other material containing VOM used in polyester resin operations, including the following polyester resin materials:

a) Corrosion resistent and fire retardant polyester resin materials used to make products for corrosive and fire retardant applications;

b) High-strength polyester resin materials with a tensile strength of 10,000 psi or more;

c) Gel coat.

(Source: Added at 18 Ill. Reg. 1253, effective January 18, 1994)