**Section 211.6020 Single-Ply Roof Membrane Installation and Repair Adhesive**

"Single-ply roof membrane installation and repair adhesive" means, for purposes of 35 Ill. Adm. Code 218 and 219, any adhesive labeled for use in the installation or repair of single-ply roof membrane. Installation includes, as a minimum, attaching the edge of the membrane to the edge of the roof and applying flashings to vents, pipes, and ducts that protrude through the membrane. Repair includes gluing the edges of A-4 torn membrane together, attaching a patch over a hole, and reapplying flashings to vents, pipes, or ducts installed through the membrane.

(Source: Added at 34 Ill. Reg. 14119, effective September 14, 2010)