**Section 211.6270 Standard Conditions**

"Standard conditions" means a temperature of 70° F and a pressure of 14.7 psia.

(Source: Added at 17 Ill. Reg. 16504, effective September 27, 1993)