**Section 212.204 Emission Units For Which Construction or Modification Commenced On or After April 14, 1972, Using Solid Fuel Exclusively**

No person shall cause or allow the emission of particulate matter into the atmosphere from any fuel combustion emission unit for which construction or modification commenced on or after April 14, 1972, using solid fuel exclusively to exceed 0.15 kg of particulate matter per MW-hr of actual heat input (0.1 lbs/mmbtu) in any one hour period unless Section 212.202, 212.203, or 212.205 applies.

(Source: Amended at 20 Ill. Reg. 7605, effective May 22, 1996)