**Section 215.181 Solvent Cleaning in General**

The requirements of Sections 215.182 through 215.184 shall not apply:

a) To sources whose emissions of volatile organic material do not exceed 6.8 kg (15 lbs) in any one day, nor 1.4 kg (3 lbs) in any one hour; or

b) To sources used exclusively for chemical or physical analysis or determination of product quality and commercial acceptance, provided that:

1) The operation of the sources is not an integral part of the production process;

2) The emissions from the source do not exceed 363 kg (800 lbs) in any calendar month; and,

3) The exemption is approved in writing by the Agency.

(Source: Amended at 3 Ill. Reg. 30, p. 124, effective July 28, 1979)