**Section 215.463 Alternative Emission Reduction Systems**

In lieu of complying with Section 215.461 or 215.462, the owner or operator of an emission source may utilize an alternative volatile organic emission reduction system, including an alternative production process, which is demonstrated to be equivalent to Section 215.461 or 215.462 on the basis of emissions of volatile organic matter. A treadend cementing operation shall be considered equivalent to Section 215.461 or 215.462 for the purposes of this Section if the total volatile organic emission from such operation is 10 grams or less per tire.

(Source: Added at 7 Ill. Reg. 1244, effective January 21, 1983)