**Section 215.484 In-Process Tanks**

The owner or operator shall install covers on all in-process tanks used to manufacture pharmaceuticals and containing a volatile organic liquid at any time. These covers must remain closed, except as production, sampling, maintenance, or inspection procedures require operator access.

(Source: Amended at 15 Ill. Reg. 8018, effective May 14, 1991)