**Section 266.135 Process Weight Rate for Catalytic Reactions, Calcining, or Other Chemical Operations**

The process weight rate for catalytic reactions, calcining, or other chemical operations is calculated by using the weight of the material added to the process. The oxygen, which chemically combines (theoretically), is allowed.