**Section 266.140 Process Weight Rate for Fluxing**

The process weight rate for fluxing is calculated by using the weight of the flux used or the make-up flux added to the bath.