**Section 276.202 Pollutants to be Tested – Exhaust Test**

Vehicle exhaust emission inspections shall consist of sampling vehicle tailpipe emissions of HC, CO, CO2, and NOx (if applicable).

(Source: Amended at 22 Ill. Reg. 18867, effective September 28, 1998)