**Section 302.303 Finished Water Standards**

Water must be of such quality that, with treatment consisting of coagulation, sedimentation, filtration, storage, and chlorination, or other equivalent treatment processes, the treated water meets all requirements of 35 Ill. Adm. Code 611.

(Source: Amended at 47 Ill. Reg. 4437, effective March 23, 2023)