**Section 310.310 Calculation of Revised Discharge Limits**

Revised discharge limits for a specific pollutant must be derived by use of the following formula:

|  |  |  |
| --- | --- | --- |
| y | = | 100x |
| (100 - r) |

where:

|  |  |  |
| --- | --- | --- |
| x | = | Pollutant discharge limit specified in the applicable categorical pretreatment standard. |
|  |  |  |
| r | = | Removal credit for the particular pollutant as established pursuant to Section 310.311 (percentage removal expressed as a percent, that is, a number between 0 and 100). |
|  |  |  |
| y | = | Revised discharge limit for the specified pollutant (expressed in same units as x). |

BOARD NOTE: Derived from 40 CFR 403.7(a)(4) (2003).

(Source: Amended at 28 Ill. Reg. 3390, effective February 6, 2004)