**Section 370.630 Pre-Aeration**

Pre-aeration of sewage to reduce septicity may be required in special cases.

(Source: Added at 21 Ill. Reg. 12444, effective August 28, 1997)