**Section 372.250 Project Layout**

A single topographic map of the proposed project and the area within 2,500 ft. of the project shall be submitted as a part of the engineering design. Segmented maps may be provided for large projects. The topographic map shall show the following information:

a) Application area boundaries including buffer zones;

b) Treatment and storage facilities;

c) Piping and layout of the irrigation system;

d) Present and proposed land use regarding residences, buildings, developments, public access areas, etc;

e) Present and proposed water supply wells and abandoned wells and shafts;

f) Direction of groundwater movement and any points of groundwater resurfacing;

g) Surface waters and waterways, wetlands and 10-year floodplains;

h) Subsurface drainage tiles and storm sewers; and

i) Slopes of the application areas.