**Section 730.163 Area of Review**

For purposes of Class I hazardous waste injection wells, this Section applies instead of Section 730.106. The area of review for a Class I hazardous waste injection well must be a two-mile radius around the well bore. The Agency may specify by permit condition a larger area of review in the UIC permit if it determines in writing that the larger area is necessary based on the calculated cone of influence of the well.

BOARD NOTE: Derived from 40 CFR 146.63 (2005).

(Source: Amended at 31 Ill. Reg. 1281, effective December 20, 2006)