**Section 732.302 No Further Action Sites**

a) Unless an owner or operator elects to classify a site under Section 732.312, sites shall be classified as No Further Action if all of the following criteria are satisfied:

1) The physical soil classification procedure completed in accordance with Section 732.307 confirms either of the following:

A) "Berg Circular"

i) The site is located in an area designated D, E, F or G on the Illinois State Geological Survey Circular (1984) entitled "Potential for Contamination of Shallow Aquifers in Illinois," incorporated by reference at Section 732.104 of this Part; and

ii) The site's actual physical soil conditions are verified as consistent with those designated D, E, F or G on the Illinois State Geological Survey Circular (1984) entitled "Potential for Contamination of Shallow Aquifers in Illinois"; or

B) The site soil characteristics satisfy the criteria of Section 732.307(d)(3) of this Part;

2) The UST system is not within the minimum or maximum setback zone of a potable water supply well or regulated recharge area of a potable water supply well;

3) After completion of early action measures in accordance with Subpart B of this Part, there is no evidence that, through natural pathways or man-made pathways, migration of petroleum or vapors threatens human health or human safety or may cause explosions in basements, crawl spaces, utility conduits, storm or sanitary sewers, vaults or other confined spaces;

4) There is no designated Class III special resource groundwater within 200 feet of the UST system; and

5) After completing early action measures in accordance with Subpart B of this Part, no surface bodies of water are adversely affected by the presence of a visible sheen or free product layer as a result of a release of petroleum.

b) Groundwater investigation shall be required to confirm that a site meets the criteria of a No Further Action site if the Agency has received information indicating that the groundwater is contaminated at levels in excess of the most stringent Tier 1 remediation objectives of 35 Ill. Adm. Code 742 for the applicable indicator contaminants at the property boundary line or 200 feet from the UST system, whichever is less. In such cases, a groundwater investigation that meets the requirements of Section 732.307(j) shall be performed. If the investigation confirms there is an exceedence of the most stringent Tier 1 remediation objectives of 35 Ill. Adm. Code 742 for the applicable indicator contaminants, the Agency may reclassify the site as High Priority.

(Source: Amended at 30 Ill. Reg. 4928, effective March 1, 2006)