**Section 811.508 Geomembranes**

The CQA officer shall exercise professional judgement to certify the following:

a) The bedding material contains no undesirable objects;

b) The placement plan has been followed;

c) The anchor trench and backfill are constructed to prevent damage to the geomembrane;

d) All tears, rips, punctures, and other damage are repaired; and

e) All geomembrane seams are properly constructed and tested in accordance with manufacturer's specifications.