**Section 817.303 Final Cover**

Unless otherwise specified in a permit or other written Agency approval, a minimum of 0.46 meters (1.5 feet) of soil material that will support vegetation which prevents or minimizes erosion shall be applied over all disturbed areas.