**Section 905.102 Noise Emission Standards**

a) No person shall operate or cause or allow the operation of a snowmobile manufactured after April 1, 1979 which generates a sound level in excess of 78 decibels on the A-scale at 50 feet when measured in accordance with procedures established under 35 Ill. Adm. Code 900.103(e)(1).

b) No person shall operate or cause or allow the operation of a snowmobile manufactured after April 1, 1979 which generates a sound level in excess of 73 decibels on the A-scale at 50 feet when measured in accordance with procedures established under 35 Ill. Adm. Code 900.103(e)(2).