**Section 160.60 Location of Tanks – Streams**

When tanks are located within 300 feet of a stream they shall be diked in conformity with Section 160.200. Existing facilities shall be brought into compliance with this rule within one year of the effective date of this rule.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)