**Section 160.400 Protection of Property – Fire Protection**

a) Fire extinguishers of at least 4A: 60 BC rating, foam generators or other agents for extinguishing oil fires shall be provided.

b) Fire extinguishers shall be installed, inspected, maintained and tested in accordance with the requirements of NFPA #10 (1981).

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)