**Section 200.504 Type 4 Magazine**

A Type 4 magazine shall be a permanent, portable or mobile structure such as a building, igloo, box, semi-trailer or other mobile containers that is fire resistant, weather resistant and ventilated, except that over-the-road trucks or semi-trailers used for temporary storage need not be ventilated or fire resistant.

a) Type 4 Outdoor Magazine.

 A Type 4 outdoor magazine shall be constructed of masonry, wood covered with metal, fabricated metal or a combination of these materials. Inside walls shall be constructed of non-sparking materials. The door shall be metal or wood covered with metal. The requirements of Section 200.501(e), (f) and (h) pertaining to foundations, floors, hinges, hardware and locks shall apply to permanent Type 4 outdoor magazines.

b) Type 4 Indoor Magazine.

 A Type 4 indoor magazines shall be constructed in accordance with the provisions for a Type 2 indoor magazine set forth in Section 200.502.

(Source: Amended at 37 Ill. Reg. 14090, effective August 26, 2013)