**Section 500.20 Definitions**

a) "ACM" means Asbestos Containing Material.

b) "Asbestos Survey Protocol" means CDB's A/E Manual of Procedures for Asbestos Inspections & Management Plans which sets forth procedures for surveying ACM in State buildings.

c) "Board" or "CDB" means the Capital Development Board.

d) "Building" means any structure used or intended for supporting or sheltering any use or occupancy.

e) "Management Plan" means a plan to provide for management of the asbestos in place, pending removal, and to establish the recommended response action.

f) "Operations and Maintenance Program" (O & M Program) means a plan of work practices to provide for the safe operation of a building with ACM, and to keep the ACM in a state of good repair. The O & M Program is a component of a Management Plan.

g) "Structure" means that which is built or constructed, an edifice or building of any kind, or any piece or work artificially built up or composed of parts joined together in some definite manner.