**Section 350.TABLE C Construction Types and Sprinkler Requirements for Existing Intermediate Care Facilities for the Developmentally Disabled**

|  |  |
| --- | --- |
| Construction Type | Stories |
| 1 | 2 | 3 | over 3 |
| 2-hour Fire Resistive | X | X |  | X |
| 1-hour Protected Noncombustible | X | X\* | X\* |  |
| Noncombustible | X\* | X\* | X\* |  |
| Heavy Timber | X\* | X\* |  |  |
| 1-hour Protected Ordinary | X\* | X\* |  |  |
| 1-hour Protected Wood Frame | X\* | X\* |  |  |
| Ordinary | X\* |  |  |  |
| Frame | X\* |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
| Key: | X | = | Allowed types of construction |  |
|  | \* | = | Building requires automatic fire extinguishment protection |