**Section 760.1130 Openings to be Protected Against Entry of Rodents and Insects**

Openings to the outside shall be effectively protected against the entry of rodents. Outside openings shall be protected against the entry of insects by tight-fitting, self-closing doors; closed windows; screening; controlled air currents; or other means. Screen doors shall be self-closing, and screens for windows, skylights, transoms, intake and exhaust air ducts, and other openings to the outside shall be tight-fitting and free of breaks. Screening material shall be not less than 16 mesh to the inch.