**Section 785.955 Lubricants**

Lubricants approved for use on milk product contact surfaces that are applied to filling machine pistons and cylinders, pumps, and valves shall be sterile (U.S.D.A. approved) and shall be applied in a sanitary manner.

(Source: Adopted at 11 Ill. Reg. 2356, effective February 1, 1987)