**Section 800.440 Abandoned Wells**

Potable water wells, borings, or monitoring wells which are abandoned shall be sealed in accordance with Section 920.120 of the Illinois Water Well Construction Code (77 Ill. Adm. Code 920).

(Source: Added at 14 Ill. Reg. 12663, effective July 20, 1990)