**Section 800.970 Unstable Refuse Bins**

Metal refuse bins having an internal volume one cubic yard or greater which will tip over when subjected to a vertical downward force of 191 pounds or a horizontal force of 70 pounds applied at a point or in a direction most likely to cause tipping shall be either removed from recreational areas or modified in such a way that they will not tip when subjected to these forces.

(Source: Amended at 4 Ill. Reg. 45, p. 147, effective October 29, 1980)