**Section 890.1030 Length and Grade**

a) Maximum Length. The maximum developed length of the indirect waste of any sanitary waste line shall not exceed 5 feet.

b) Grade. Indirect waste pipes shall be installed at a uniform grade, in compliance with Section 890.1320(f), (g) and (h).

(Source: Amended at 28 Ill. Reg. 4215, effective February 18, 2004)