**Section 890.APPENDIX A**  **Plumbing Materials, Equipment, Use Restrictions and Applicable Standards**

**Section 890.TABLE I**  **Allowed Distance from Fixture Trap to Vent**

|  |  |  |
| --- | --- | --- |
| Size of Fixture Drains (Inches) |  | Maximum Allowed Distance from Trap to Vent |
| 1¼ |  | 2 ft. 6 in. |
| 1½ |  | 3 ft. 6 in. |
| 2 |  | 4 ft. 0 in. |
| 3 |  | 5 ft. 0 in. |
| 4 and larger |  | 6 ft. 0 in. |