**Section 1110.APPENDIX B State Guidelines − Square Footage and Utilization**

The following area standards are established for departments, clinical service areas and facilities. All Diagnostic and Treatment utilization numbers are the minimums per unit for establishing more than one unit, except where noted in 77 Ill. Adm. Code 1100. HFSRB shall periodically evaluate the guidelines to determine if revisions should be made. Any revisions will be promulgated in accordance with the provisions of the Illinois Administrative Procedure Act.

Definitions pertaining to this Appendix are contained in 77 Ill. Adm. Code 1100.220.

HOSPITAL-BASED SERVICES

For hospitals, area determinations for departments and clinical service areas are to be made in departmental gross square feet (dgsf). Spaces to be included in the applicant's determination of square footage shall include all functional areas minimally required by the Hospital Licensing Act, applicable federal certification, and any additional spaces required by the applicant's operational program.

|  |  |  |
| --- | --- | --- |
| **Service Areas** | **Square Feet/Unit or Key Room** | **Annual Utilization/Unit** |
| Acute Care |  |  |
| Medical-Surgical, Pediatric, Obstetric & Long Term Acute Care Service | 500-660 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| Newborn Nursery (includes Level I, Level II, and Level II+ with extended neonatal capabilities) | 160 dgsf/Obstetrics Bed & LDRP |  |
| Labor Delivery Recovery (LDR) | 1120-1600 dgsf/Room | 400 Births/LDR Room |
| Labor Delivery Recovery Post-partum (LDRP) | 1120-1600 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| C-Section Suite | 2075 dgsf/OR | 800 Procedures/Room |
| Acute Mental Illness Service | 440-560 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| Comprehensive Physical Rehabilitation Service | 525-660 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| Hospital Based Long-Term Care | 440-560 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| Critical Care |  |  |
| Intensive Care Service | 600-685 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| Neonatal Intensive Care (NICU) or Level III Nursery | 434-568 dgsf/Bed or Bassinet | See 77 Ill. Adm. Code 1100 |
| Diagnostic and Treatment |  |  |
| Diagnostic/Interventional Radiology (Excludes portables & mobile equipment/Utilization) |  |  |
| • General Radiology | 1300 dgsf/Unit | 8000 procedures |
| • Fluoroscopy/Tomography/Other  X-ray procedures | 1300 dgsf/Unit | 6500 procedures |
| • Dedicated Chest | 900 dgsf/Unit | 9000 procedures |
| • Mammography | 900 dgsf/Unit | 5000 visits |
| • Ultra-Sound | 900 dgsf/Unit | 3100 visits |
| • Angiography (Special Procedures) | 1800 dgsf/Unit | 1800 visits |
| • CT Scan | 1800 dgsf/Unit | 7000 visits |
| • PET | 1800 dgsf/Unit | 3600 visits |
| • MRI | 1800 dgsf/Unit | 2500 procedures |
| • Nuclear Medicine | 1600 dgsf/Unit | 2000 visits |
| Radiation Therapy |  |  |
| • Accelerator | 2400 dgsf/  Accelerator | 7500 treatments |
| • Simulator | 1800 dgsf/  Simulator |  |
| Emergency Department | 900 dgsf/ Treatment Station | 2000 visits/station/year |
| Cardiac Catheterization | 1800 dgsf | See 77 Ill. Adm. Code 1100 for establishment of service 1500 visits/year for additional units |
| Ambulatory Care | 800 dgsf | 2000 visits/year |
| Surgical Operating Suite (Class C) | 2750 dgsf/  Operating Room | 1500 hrs/Operating Room |
| Surgical Procedure Suite (Class B) | 1100 dgsf/  Procedure Room | 1500 hrs/Procedure Room |
| Post-Anesthesia Recovery Phase I | 180 dgsf/Recovery Station |  |
| Post-Anesthesia Recovery Phase II | 400 dgsf/Recovery Station |  |
| In-Center Hemodialysis | 470 dgsf/Station | See 77 Ill. Adm. Code 1100 |

HFSRB NOTE: The standards for Post-Anesthesia Recovery Phase I and Post-Anesthesia Recovery Phase II shall be used as the standards for recovery stations associated with Surgical Operating Suite (Class C) and Surgical Procedure Suite (Class B).

OTHER FACILITIES

The following standards apply to new construction, the development of freestanding facilities, modernization, and the development of facilities in existing structures, including the use of leased space. For new construction, the standards are based upon the inclusion of all building components and are expressed in building gross square feet (bgsf). For modernization projects, the standards are based upon interior build-out only and are expressed in departmental gross square feet (dgsf). Spaces to be included in the applicant's determination of square footage shall include all functional areas minimally required for the applicable service areas by the appropriate rules required for IDPH licensure and/or federal certification and any additional spaces required by the applicant's operational program.

|  |  |  |
| --- | --- | --- |
| **Service Areas** | **Square Feet/Unit** | **Annual Utilization/Unit** |
| General Long Term Care | 435-713 bgsf/Bed  350-570 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| ICF/DD Facilities | 505-580 bgsf/Bed  404-464 dgsf/Bed | See 77 Ill. Adm. Code 1100 |
| Ambulatory Surgical Treatment Center (ASTC) | 2075-2750 bgsf/Treatment Room  1660-2200 dgsf/Treatment Room | Maximum of 4 recovery stations per operating room 1500 hrs of Surgery/OR or Procedure Room |
| • Operating Room |
| • Procedure Room |
| • Recovery |
| In-Center Hemodialysis | 450-650  bgsf/Room  360-520 dgsf/Room | See 77 Ill. Adm. Code 1100 |
| Freestanding Emergency Center | 840-1170 bgsf/Treatment Station  672-936 dgsf/Treatment Station | 2000 visits/Treatment Room/year |